**Pricing Tables**

Table # **–** Fibre Optic Conduit Items

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item # | Item Description | Unit of Measurement | Estimated Quantity | Unit Price | Total |
| F101 | Supply and Install 50 mm Diameter Rigid DB2 PVC Conduit by Open Cut (Traffic Controller Handholes) | metres |  |  |  |
| F102 | Supply and Install 1 x 2.03 inches (51.6 mm) Diameter 7-Way HDPE Bundled 16/12 mm Microducts by Open Cut | metres |  |  |  |
| F102 | Supply and Install 2 x 2.03 inches (51.6 mm) Diameter 7-Way HDPE Bundled 16/12 mm Microducts by Open Cut | metres |  |  |  |
| F102 | Supply and Install 3 x 2.03 inches (51.6 mm) Diameter 7-Way HDPE Bundled 16/12 mm Microducts by Open Cut | metres |  |  |  |
| F103 | Supply and Install 1 x 2.03 inches (51.6 mm) Diameter 7-Way HDPE Bundled 16/12 mm Microducts by Directional Bore | metres |  |  |  |
| F103 | Supply and Install 2 x 2.03 inches (51.6 mm) Diameter 7-Way HDPE Bundled 16/12 mm Microducts by Directional Bore | metres |  |  |  |
| F103 | Supply and Install 3 x 2.03 inches (51.6 mm) Diameter 7-Way HDPE Bundled 16/12 mm Microducts by Directional Bore | metres |  |  |  |
| F104 | Supply and Install 50 mm Diameter Coilable HDPE Conduit by Directional Bore | metres |  |  |  |
| F105 | Supply and Install 30 inches x 48 inches x 36 inches Polymer Concrete Vault with Lid | each |  |  |  |
| F106 | Break into Existing Traffic Handwell | each |  |  |  |
| F107 | Break into Existing Vault | each |  |  |  |