**The information in this document is information that we will be entering directly onto the Bids and Tenders website.**

**Pre-Qualified Subcontractors**

*If Subcontractors were pre-qualified for this Contract please complete this following section.*

*Please duplicate the language as many times as necessary (e.g. if you have pre-qualified Electrical and Mechanical Subcontractors this section should be completed once for the Electrical Subcontractors and a second time for the Mechanical Subcontractors).*

*DON’T TRY TO CONSOLIDATE THE LANGUAGE. We will be building individual tables for each type of pre-qualified Subcontractors on the Bids and Tenders website and each table will have its own introductory language.*

**Subcontractors**

The following is a list of pre-qualified       Subcontractors that have been approved to carry out the       work under this Contract, as qualified under Request for Pre-Qualification No.      .

Bidders must list one of the       Subcontractors pre-qualified under Request for Pre-Qualification No.       (as identified below) for the       component of the Work.

**Any bids that fail to meet this requirement shall be rejected from further consideration.**

*

**Bidders Meeting**

*If you require a Bidders Meeting please provide the following information:*

Date of Meeting:

Time of Meeting:

Location of Meeting:

**Pricing Tables**

Table # – General Contract Items

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item # | Item Description | Unit of Measurement | Estimated Quantity | Unit Price | Total |
| G1 | Maintenance of Traffic | lump sum | 1 |  |  |
| G2 | Construction Layout | lump sum | 1 |  |  |
| G3 | Provision of On-Site Facilities | lump sum | 1 |  |  |
| G4 | Environmental Protection | lump sum | 1 |  |  |
| G5 | Full Matrix Portable Variable Message Signs (PVMS) | sign Days |  |  |  |

**Lane Rentals**

A procedure known as “lane rental” is being used on this Contract to decrease the impact of construction on road users.

Under this item, lane rental charges will be assessed for the time, in hours, that the Contractor requires lanes to be closed to traffic (“Lane Hours”). Lane Hours will be measured for each hour, or part thereof, that a lane, or part thereof, is closed to traffic, and will be rounded up to the nearest hour. For example, two (2) traffic lanes closed for 10 hours will total 20 Lane Hours (10 Lane Hours per lane). Bidders should refer to the Specifications for a detailed description of how lane rental charges will be assessed under this item.

As part of their bids, Bidders shall enter the number of Lane Hours they require in order to complete the Work in the table below:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Item # | Item Description | Unit of Measurement | Estimated Quantity | Unit Price | Total |
| G6 | Lane Rental  | hours |  | 200.00 |  |